[ForceFW]

//---
/FLASH_45D7988276D5_ISP=SM3257ENAAISP-ISPSDEX3.BIN
/FLASH_45D7988276D5_PTEST=SM3257ENAATSPTEST.bin
/FLASH_45D7988276D5_DisableCardModeFW=1
//---
/FLASH_45DEA8827A55_ISP=SM3257ENAAISP-ISPSDEX3.BIN
/FLASH_45DEA8827A55_PTEST=SM3257ENAATSPTEST.bin
/FLASH_45DEA8827A55_DisableCardModeFW=1
//---
/FLASH_45DEA8827AD5_ISP=SM3257ENAAISP-ISPSDEX3.BIN
/FLASH_45DEA8827AD5_PTEST=SM3257ENAATSPTEST.bin
/FLASH_45DEA8827AD5_DisableCardModeFW=1
//---
/FLASH_45D588827255_ISP=SM3257ENAAISP-ISPSDEX3.BIN
/FLASH_45D588827255_PTEST=SM3257ENAATSPTEST.bin
/FLASH_45D588827255_DisableCardModeFW=1
//---
/FLASH_45D798827655_ISP=SM3257ENAAISP-ISPSDEX3.BIN
/FLASH_45D798827655_PTEST=SM3257ENAATSPTEST.bin
/FLASH_45D798827655_DisableCardModeFW=1
//---
/FLASH_45CEA8827AD5_ISP=SM3257ENAAISP-ISPSDEX3.BIN
/FLASH_45CEA8827AD5_PTEST=SM3257ENAATSPTEST.bin
/FLASH_45CEA8827AD5_DisableCardModeFW=1
//---
/FLASH_98D798827655_ISP=SM3257ENAAISP-ISPTEX3.BIN
/FLASH_98D798827655_PTEST=SM3257ENAATSPTEST.bin
/FLASH_98D798827655_DisableCardModeFW=1
//---
/FLASH_989798827655_ISP=SM3257ENAAISP-ISPTEX3.BIN
/FLASH_989798827655_PTEST=SM3257ENAATSPTEST.bin
/FLASH_989798827655_DisableCardModeFW=1
//---
/FLASH_98D588827255_ISP=SM3257ENAAISP-ISPTEX3.BIN
/FLASH_98D588827255_PTEST=SM3257ENAATSPTEST.bin
/FLASH_98D588827255_DisableCardModeFW=1
//---
/FLASH_98DEA8827A55_ISP=SM3257ENAAISP-ISPTEX3.BIN
/FLASH_98DEA8827A55_PTEST=SM3257ENAATSPTEST.bin
/FLASH_98DEA8827A55_DisableCardModeFW=1
//---
/FLASH_98DEA8827AD5_ISP=SM3257ENAAISP-ISPTEX3.BIN
/FLASH_98DEA8827AD5_PTEST=SM3257ENAATSPTEST.bin
/FLASH_98DEA8827AD5_DisableCardModeFW=1
//---
/FLASH_98D7988276D5_ISP=SM3257ENAAISP-ISPTEX3.BIN
/FLASH_98D7988276D5_PTEST=SM3257ENAATSPTEST.bin
/FLASH_98D7988276D5_DisableCardModeFW=1
//---
/FLASH_45C798B276D5_ISP=SM3257ENAAISP-ISPSDEX3.BIN
/FLASH_45C798B276D5_PTEST=SM3257ENAATSPTEST.bin
/FLASH_45C798B276D5_DisableCardModeFW=1
//---
/FLASH_45D798B276D5_ISP=SM3257ENAAISP-ISPSDEX3.BIN
/FLASH_45D798B276D5_PTEST=SM3257ENAATSPTEST.bin
/FLASH_45D798B276D5_DisableCardModeFW=1
//---
/FLASH_454A9AB27ED5_ISP=SM3257ENAAISP-ISPSDEX3_Qual.BIN
/FLASH_454A9AB27ED5_PTEST=SM3257ENAATSPTEST_Qual.bin
/FLASH_454A9AB27ED5_DisableCardModeFW=1
//---
/FLASH_984A9AB27ED5_ISP=SM3257ENAAISP-ISPTEX3_Qual.BIN
/FLASH_984A9AB27ED5_PTEST=SM3257ENAATSPTEST_Qual.bin
/FLASH_984A9AB27ED5_DisableCardModeFW=1
//---
FLASH_98DE98927256_ISP=SM3267ACISP-ISPT24nm.BIN
FLASH_98DE98927256_PTEST=SM3267ACPTEST.bin
FLASH_98DE98927256_DisableCardModeFW=1
//---
FLASH_98DE989272D6_ISP=SM3267ACISP-ISPT24nm.BIN
FLASH_98DE989272D6_PTEST=SM3267ACPTEST.bin
FLASH_98DE989272D6_DisableCardModeFW=1
//---
FLASH_98D798927256_ISP=SM3267ACISP-ISPT24nm.BIN
FLASH_98D798927256_PTEST=SM3267ACPTEST.bin
FLASH_98D798927256_DisableCardModeFW=1
//---
FLASH_98D7989272D6_ISP=SM3260ADISP-ISPT24nm.BIN
FLASH_98D7989272D6_PTEST=SM3267ACPTEST.bin
FLASH_98D7989272D6_DisableCardModeFW=1
//---
FLASH_983A99927656_ISP=SM3267ACISP-ISPT24nm.BIN
FLASH_983A99927656_PTEST=SM3267ACPTEST.bin
FLASH_983A99927656_DisableCardModeFW=1
//---
FLASH_98DE999276D6_ISP=SM3267ACISP-ISPT24nm.BIN
FLASH_98DE999276D6_PTEST=SM3267ACPTEST.bin
FLASH_98DE999276D6_DisableCardModeFW=1
//---
FLASH_45DE98927256_ISP=SM3267ACISP-ISPSD24nm.BIN
FLASH_45DE98927256_PTEST=SM3267ACPTEST.bin
FLASH_45DE98927256_DisableCardModeFW=1
//---
FLASH_45D798927256_ISP=SM3267ACISP-ISPSD24nm.BIN
FLASH_45D798927256_PTEST=SM3267ACPTEST.bin
FLASH_45D798927256_DisableCardModeFW=1
//---
FLASH_45DE989272D6_ISP=SM3267ACISP-ISPSD24nm.BIN
FLASH_45DE989272D6_PTEST=SM3267ACPTEST.bin
FLASH_45DE989272D6_DisableCardModeFW=1
//---
FLASH_45D7989272D6_ISP=SM3267ACISP-ISPSD24nm.BIN
FLASH_45D7989272D6_PTEST=SM3267ACPTEST.bin
FLASH_45D7989272D6_DisableCardModeFW=1
//---
FLASH_45DE98927257_ISP=SM3267ACISP-ISPSD19nm.BIN
FLASH_45DE98927257_PTEST=SM3267ACPTEST.bin
FLASH_45DE98927257_DisableCardModeFW=1
//---
FLASH_98DE98927257_ISP=SM3267ACISP-ISPT19nm.BIN
FLASH_98DE98927257_PTEST=SM3267ACPTEST.bin
FLASH_98DE98927257_DisableCardModeFW=1
//---
FLASH_98DE989272D7_ISP=SM3267ACISP-ISPT19nm.BIN
FLASH_98DE989272D7_PTEST=SM3267ACPTEST.bin
FLASH_98DE989272D7_DisableCardModeFW=1
//---
FLASH_98D798927257_ISP=SM3267ACISP-ISPT19nm.BIN
FLASH_98D798927257_PTEST=SM3267ACPTEST.bin
FLASH_98D798927257_DisableCardModeFW=1
//---
FLASH_98D7989272D7_ISP=SM3267ACISP-ISPT19nm.BIN
FLASH_98D7989272D7_PTEST=SM3267ACPTEST.bin
FLASH_98D7989272D7_DisableCardModeFW=1
//---
FLASH_45DE98927250_ISP=SM3267ACISP-ISPSDA19nm.BIN
FLASH_45DE98927250_PTEST=SM3267ACPTEST.bin
FLASH_45DE98927250_DisableCardModeFW=1
//---
FLASH_45DE989272D0_ISP=SM3267ACISP-ISPSDA19nm.BIN
FLASH_45DE989272D0_PTEST=SM3267ACPTEST.bin
FLASH_45DE989272D0_DisableCardModeFW=1
//---
FLASH_45DEA8927650_ISP=SM3267ACISP-ISPSDA19nm.BIN
FLASH_45DEA8927650_PTEST=SM3267ACPTEST.bin
FLASH_45DEA8927650_DisableCardModeFW=1
//---
FLASH_45DEA89276D0_ISP=SM3267ACISP-ISPSDA19nm.BIN
FLASH_45DEA89276D0_PTEST=SM3267ACPTEST.bin
FLASH_45DEA89276D0_DisableCardModeFW=1
//---
FLASH_454CA8927650_ISP=SM3267ACISP-ISPSDA19nm.BIN
FLASH_454CA8927650_PTEST=SM3267ACPTEST.bin
FLASH_454CA8927650_DisableCardModeFW=1
//---
FLASH_454CA89276D0_ISP=SM3267ACISP-ISPSDA19nm.BIN
FLASH_454CA89276D0_PTEST=SM3267ACPTEST.bin
FLASH_454CA89276D0_DisableCardModeFW=1
//---
FLASH_98DE98927250_ISP=SM3267ACISP-ISPTA19nm.BIN
FLASH_98DE98927250_PTEST=SM3267ACPTEST.bin
FLASH_98DE98927250_DisableCardModeFW=1
//---
FLASH_98DE989272D0_ISP=SM3267ACISP-ISPTA19nm.BIN
FLASH_98DE989272D0_PTEST=SM3267ACPTEST.bin
FLASH_98DE989272D0_DisableCardModeFW=1
//---
FLASH_983AA8927650_ISP=SM3267ACISP-ISPTA19nm.BIN
FLASH_983AA8927650_PTEST=SM3267ACPTEST.bin
FLASH_983AA8927650_DisableCardModeFW=1
//---
FLASH_983AA89276D0_ISP=SM3267ACISP-ISPTA19nm.BIN
FLASH_983AA89276D0_PTEST=SM3267ACPTEST.bin
FLASH_983AA89276D0_DisableCardModeFW=1
//---
FLASH_98DE88A37251_ISP=SM3267ACISP-ISPT15nmTLC.BIN
FLASH_98DE88A37251_PTEST=SM3267ACPTEST.bin
FLASH_98DE88A37251_DisableCardModeFW=1
//---
FLASH_983A98A37651_ISP=SM3267ACISP-ISPT15nmTLC.BIN
FLASH_983A98A37651_PTEST=SM3267ACPTEST.bin
FLASH_983A98A37651_DisableCardModeFW=1
//---
FLASH_454C98A37651_ISP=SM3267ACISP-ISPSD15nmTLC.BIN
FLASH_454C98A37651_PTEST=SM3267ACPTEST.bin
FLASH_454C98A37651_DisableCardModeFW=1
//---
FLASH_ECDE98CE74C4_ISP=SM3267ACISP-ISPSA21nm.BIN
FLASH_ECDE98CE74C4_PTEST=SM3267ACPTEST.bin
FLASH_ECDE98CE74C4_DisableCardModeFW=1
//---
FLASH_ECD598CE74C4_ISP=SM3267ACISP-ISPSA21nm.BIN
FLASH_ECD598CE74C4_PTEST=SM3267ACPTEST.bin
FLASH_ECD598CE74C4_DisableCardModeFW=1
//---
FLASH_ECD798CE74C4_ISP=SM3267ACISP-ISPSA21nm.BIN
FLASH_ECD798CE74C4_PTEST=SM3267ACPTEST.bin
FLASH_ECD798CE74C4_DisableCardModeFW=1
//---
FLASH_EC3AD9CE78C4_ISP1=SM3267ACISP-ISPSA21nm2die.BIN
FLASH_EC3AD9CE78C4_PTEST1=SM3267ACPTEST.bin
FLASH_EC3AD9CE78C4_ISP2=SM3267ACISP-ISPSA21nm2die.BIN
FLASH_EC3AD9CE78C4_PTEST2=SM3267ACPTEST.bin
FLASH_EC3AD9CE78C4_ISP4=SM3267ACISP-ISPSA21nm2die.BIN
FLASH_EC3AD9CE78C4_PTEST4=SM3267ACPTEST.bin
FLASH_EC3AD9CE78C4_DisableCardModeFW=1
//---
FLASH_EC1AA8DE88C5_ISP=SM3267ACISP-ISPSA19nm.BIN
FLASH_EC1AA8DE88C5_PTEST=SM3267ACPTEST.bin
FLASH_EC1AA8DE88C5_PSCAN=SM3267ACPSCN.bin
FLASH_EC1AA8DE88C5_DisableCardModeFW=1
FLASH_EC1AA8DE88C5_EMICLK=1
//---
FLASH_ECD598DE94C5_ISP=SM3267ACISP-ISPSA19nm.BIN
FLASH_ECD598DE94C5_PTEST=SM3267ACPTEST.bin
/FLASH_ECD598DE94C5_PSCAN=SM3267ACPSCN.bin
FLASH_ECD598DE94C5_DisableCardModeFW=1
FLASH_ECD598DE94C5_EMICLK=1
//---
FLASH_ECDE98DE94C5_ISP=SM3267ACISP-ISPSA19nm.BIN
FLASH_ECDE98DE94C5_PTEST=SM3267ACPTEST.bin
FLASH_ECDE98DE94C5_PSCAN=SM3267ACPSCN.bin
FLASH_ECDE98DE94C5_DisableCardModeFW=1
FLASH_ECDE98DE94C5_EMICLK=1
//---
FLASH_ECD798DE94C5_ISP=SM3267ACISP-ISPSA19nm.BIN
FLASH_ECD798DE94C5_PTEST=SM3267ACPTEST.bin
FLASH_ECD798DE94C5_PSCAN=SM3267ACPSCN.bin
FLASH_ECD798DE94C5_DisableCardModeFW=1
FLASH_ECD798DE94C5_EMICLK=1
//---
FLASH_ECD598DE94C5_ISP=SM3267ACISP-ISPSA19nm.BIN
FLASH_ECD598DE94C5_PTEST=SM3267ACPTEST.bin
FLASH_ECD598DE94C5_PSCAN=SM3267ACPSCN.bin
FLASH_ECD598DE94C5_DisableCardModeFW=1
FLASH_ECD598DE94C5_EMICLK=1
//---
FLASH_ECD788BF90C6_ISP=SM3267ACISP-ISPSAA19nm.BIN
FLASH_ECD788BF90C6_PTEST=SM3267ACPTEST.bin
FLASH_ECD788BF90C6_DisableCardModeFW=1
//---
FLASH_ECDE88BF90C6_ISP=SM3267ACISP-ISPSAA19nm.BIN
FLASH_ECDE88BF90C6_PTEST=SM3267ACPTEST.bin
FLASH_ECDE88BF90C6_DisableCardModeFW=1
//---
FLASH_EC3A98BF94C6_ISP=SM3267ACISP-ISPSAA19nm.BIN
FLASH_EC3A98BF94C6_PTEST=SM3267ACPTEST.bin
FLASH_EC3A98BF94C6_DisableCardModeFW=1
//---
FLASH_EC0000DE00C5_ISP=SM3267ACISP-ISPSA19nm2die.BIN
FLASH_EC0000DE00C5_PTEST=SM3267ACPTEST.bin
FLASH_EC0000DE00C5_DisableCardModeFW=1
FLASH_EC0000DE00C5_EMICLK=1
//---
FLASH_EC3CE9DE88C5_ISP=SM3267ACISP-ISPSA19nm2die.BIN
FLASH_EC3CE9DE88C5_PTEST=SM3267ACPTEST.bin
FLASH_EC3CE9DE88C5_DisableCardModeFW=1
FLASH_EC3CE9DE88C5_EMICLK=1
//---
FLASH_EC3AD9DE94C5_ISP=SM3267ACISP-ISPSA19nm2die.BIN
FLASH_EC3AD9DE94C5_PTEST=SM3267ACPTEST.bin
FLASH_EC3AD9DE94C5_DisableCardModeFW=1
FLASH_EC3AD9DE94C5_EMICLK=1
//---
//---
FLASH_ECAEB8DE86C5_ISP=SM3267ACISP-ISPSA19nm3P.BIN
FLASH_ECAEB8DE86C5_PTEST=SM3267ACPTEST.bin
FLASH_ECAEB8DE86C5_PSCAN=SM3267ACPSCN.bin
FLASH_ECAEB8DE86C5_DisableCardModeFW=1
FLASH_ECAEB8DE86C5_EMICLK=1
//---


//---
FLASH_983AA8927657_ISP=SM3267ACISP-ISPT19nm.BIN
FLASH_983AA8927657_PTEST=SM3267ACPTEST.bin
FLASH_983AA8927657_DisableCardModeFW=1
//---
FLASH_983AA89276D7_ISP=SM3267ACISP-ISPT19nm.BIN
FLASH_983AA89276D7_PTEST=SM3267ACPTEST.bin
FLASH_983AA89276D7_DisableCardModeFW=1
//---
FLASH_983CA9927A57_ISP1=SM3267ACISP-ISPT19nm2die.BIN
FLASH_983CA9927A57_PTEST1=SM3267ACPTEST.bin
FLASH_983CA9927A57_ISP2=SM3267ACISP-ISPT19nm2die.BIN
FLASH_983CA9927A57_PTEST2=SM3267ACPTEST.bin
FLASH_983CA9927A57_ISP4=SM3267ACISP-ISPT19nm2die.BIN
FLASH_983CA9927A57_PTEST4=SM3267ACPTEST.bin
FLASH_983CA9927A57_DisableCardModeFW=1
//---
FLASH_EC3CD9BF98C6_ISP=SM3267ACISP-ISPSAA19nm_2DN.BIN
FLASH_EC3CD9BF98C6_PTEST=SM3267ACPTEST.bin
FLASH_EC3CD9BF98C6_DisableCardModeFW=1
//---
FLASH_EC3AC9BF94C6_ISP=SM3267ACISP-ISPSAA19nm_2DN.BIN
FLASH_EC3AC9BF94C6_PTEST=SM3267ACPTEST.bin
FLASH_EC3AC9BF94C6_DisableCardModeFW=1
//---
FLASH_983CA9927A50_ISP1=SM3267ACISP-ISPTA19nm_2DN.BIN
FLASH_983CA9927A50_PTEST1=SM3267ACPTEST.bin
FLASH_983CA9927A50_ISP2=SM3267ACISP-ISPTA19nm_2DN.BIN
FLASH_983CA9927A50_PTEST2=SM3267ACPTEST.bin
FLASH_983CA9927A50_ISP4=SM3267ACISP-ISPTA19nm_2DN.BIN
FLASH_983CA9927A50_PTEST4=SM3267ACPTEST.bin
FLASH_983CA9927A50_DisableCardModeFW=1
//---
FLASH_983CA9927AD0_ISP1=SM3267ACISP-ISPTA19nm_2DN.BIN
FLASH_983CA9927AD0_PTEST1=SM3267ACPTEST.bin
FLASH_983CA9927AD0_ISP2=SM3267ACISP-ISPTA19nm_2DN.BIN
FLASH_983CA9927AD0_PTEST2=SM3267ACPTEST.bin
FLASH_983CA9927AD0_ISP4=SM3267ACISP-ISPTA19nm_2DN.BIN
FLASH_983CA9927AD0_PTEST4=SM3267ACPTEST.bin
FLASH_983CA9927AD0_DisableCardModeFW=1
//---
FLASH_983DA9927A50_ISP=SM3267ACISP-ISPTA19nm_2DN.BIN
FLASH_983DA9927A50_PTEST=SM3267ACPTEST.bin
FLASH_983DA9927A50_DisableCardModeFW=1
//---
FLASH_454CA8927657_ISP=SM3267ACISP-ISPSD19nm.BIN
FLASH_454CA8927657_PTEST=SM3267ACPTEST.bin
FLASH_454CA8927657_DisableCardModeFW=1
//---
FLASH_453CA9927A57_ISP1=SM3267ACISP-ISPSD19nm2die.BIN
FLASH_453CA9927A57_PTEST1=SM3267ACPTEST.bin
FLASH_453CA9927A57_ISP2=SM3267ACISP-ISPSD19nm2die.BIN
FLASH_453CA9927A57_PTEST2=SM3267ACPTEST.bin
FLASH_453CA9927A57_ISP4=SM3267ACISP-ISPSD19nm2die.BIN
FLASH_453CA9927A57_PTEST4=SM3267ACPTEST.bin
FLASH_453CA9927A57_DisableCardModeFW=1
//---
FLASH_45D798927257_ISP=SM3267ACISP-ISPSD19nm.BIN
FLASH_45D798927257_PTEST=SM3267ACPTEST.bin
FLASH_45D798927257_DisableCardModeFW=1
//---

//---
FLASH_2C9805CF8900_ISP=SM3267ACISP.bin
FLASH_2C9805CF8900_PTEST=SM3267ACPTEST.bin
FLASH_2C9805CF8900_PSCAN=SM3267ACPSCN.bin
FLASH_2C9805CF8900_PSCNFlash=3
FLASH_2C9805CF8900_DisableCardModeFW=1
//---
FLASH_8988243BA900_ISP=SM3267ACISP.bin
FLASH_8988243BA900_PTEST=SM3267ACPTEST.bin
FLASH_8988243BA900_PSCAN=SM3267ACPSCN.bin
FLASH_8988243BA900_PSCNFlash=3
FLASH_8988243BA900_DisableCardModeFW=1
//---
FLASH_2C88044BA900_ISP=SM3267ACISP.bin
FLASH_2C88044BA900_PTEST=SM3267ACPTEST.bin
FLASH_2C88044BA900_PSCAN=SM3267ACPSCN.bin
FLASH_2C88044BA900_PSCNFlash=3
FLASH_2C88044BA900_DisableCardModeFW=1
//---
FLASH_2C8824498900_ISP=SM3267ACISP.bin
FLASH_2C8824498900_PTEST=SM3267ACPTEST.bin
FLASH_2C8824498900_PSCAN=SM3267ACPSCN.bin
FLASH_2C8824498900_PSCNFlash=3
FLASH_2C8824498900_DisableCardModeFW=1
//---
FLASH_2C88244BA900_ISP=SM3267ACISP.bin
FLASH_2C88244BA900_PTEST=SM3267ACPTEST.bin
FLASH_2C88244BA900_PSCAN=SM3267ACPSCN.bin
FLASH_2C88244BA900_PSCNFlash=3
FLASH_2C88244BA900_DisableCardModeFW=1
//---
FLASH_2CA805CBA900_ISP=SM3267ACISP.bin
FLASH_2CA805CBA900_PTEST=SM3267ACPTEST.bin
FLASH_2CA805CBA900_PSCAN=SM3267ACPSCN.bin
FLASH_2CA805CBA900_PSCNFlash=3
FLASH_2CA805CBA900_DisableCardModeFW=1
//---
FLASH_2CA825CB8900_ISP=SM3267ACISP.bin
FLASH_2CA825CB8900_PTEST=SM3267ACPTEST.bin
FLASH_2CA825CB8900_PSCAN=SM3267ACPSCN.bin
FLASH_2CA825CB8900_PSCNFlash=3
FLASH_2CA825CB8900_DisableCardModeFW=1
//---
FLASH_89882449A900_ISP=SM3267ACISP.bin
FLASH_89882449A900_PTEST=SM3267ACPTEST.bin
FLASH_89882449A900_PSCAN=SM3267ACPSCN.bin
FLASH_89882449A900_PSCNFlash=3
FLASH_89882449A900_DisableCardModeFW=1
//---
FLASH_8988244BA900_ISP=SM3267ACISP.bin
FLASH_8988244BA900_PTEST=SM3267ACPTEST.bin
FLASH_8988244BA900_PSCAN=SM3267ACPSCN.bin
FLASH_8988244BA900_PSCNFlash=3
FLASH_8988244BA900_DisableCardModeFW=1
//---
FLASH_8988044BA900_ISP=SM3267ACISP.bin
FLASH_8988044BA900_PTEST=SM3267ACPTEST.bin
FLASH_8988044BA900_PSCAN=SM3267ACPSCN.bin
FLASH_8988044BA900_PSCNFlash=3
FLASH_8988044BA900_DisableCardModeFW=1
//---
FLASH_89A825CBA900_ISP=SM3267ACISP.bin
FLASH_89A825CBA900_PTEST=SM3267ACPTEST.bin
FLASH_89A825CBA900_PSCAN=SM3267ACPSCN.bin
FLASH_89A825CBA900_PSCNFlash=3
FLASH_89A825CBA900_DisableCardModeFW=1
//---
FLASH_89C826CBA900_ISP=SM3267ACISP.bin
FLASH_89C826CBA900_PTEST=SM3267ACPTEST.bin
FLASH_89C826CBA900_PSCAN=SM3267ACPSCN.bin
FLASH_89C826CBA900_PSCNFlash=3
FLASH_89C826CBA900_DisableCardModeFW=1
//---
FLASH_2C78044F8900_ISP=SM3267ACISP.bin
FLASH_2C78044F8900_PTEST=SM3267ACPTEST.bin
FLASH_2C78044F8900_PSCAN=SM3267ACPSCN.bin
FLASH_2C78044F8900_PSCNFlash=3
FLASH_2C78044F8900_DisableCardModeFW=1
//---


//---
FLASH_2C88085FA900_ISP=SM3267ACISP-B74.bin
FLASH_2C88085FA900_PTEST=SM3267ACPTEST.bin
FLASH_2C88085FA900_DisableCardModeFW=1
//---
FLASH_2C88285FA900_ISP=SM3267ACISP-B74.bin
FLASH_2C88285FA900_PTEST=SM3267ACPTEST.bin
FLASH_2C88285FA900_DisableCardModeFW=1
//---
FLASH_8988285FA900_ISP=SM3267ACISP-B74.bin
FLASH_8988285FA900_PTEST=SM3267ACPTEST.bin
FLASH_8988285FA900_DisableCardModeFW=1
//---
FLASH_2CA809DFA900_ISP=SM3267ACISP-B74.bin
FLASH_2CA809DFA900_PTEST=SM3267ACPTEST.bin
FLASH_2CA809DFA900_DisableCardModeFW=1
//---
FLASH_2C88085F8900_ISP=SM3267ACISP-B74.bin
FLASH_2C88085F8900_PTEST=SM3267ACPTEST.bin
FLASH_2C88085F8900_DisableCardModeFW=1
//---
FLASH_2CA809DF8900_ISP=SM3267ACISP-B74.bin
FLASH_2CA809DF8900_PTEST=SM3267ACPTEST.bin
FLASH_2CA809DF8900_DisableCardModeFW=1
//---
FLASH_ECDE98CE74C3_ISP=SM3267ACISP-27nm.BIN
FLASH_ECDE98CE74C3_PTEST=SM3267ACPTEST.bin
FLASH_ECDE98CE74C3_DisableCardModeFW=1
//---
FLASH_EC3AD9CE78C3_ISP=SM3267ACISP-27nm.BIN
FLASH_EC3AD9CE78C3_PTEST=SM3267ACPTEST.bin
FLASH_EC3AD9CE78C3_DisableCardModeFW=1
//---
FLASH_ECD798CA5442_ISP=SM3267ACISP-bucket01.BIN
FLASH_ECD798CA5442_PTEST=SM3267ACPTEST.bin
FLASH_ECD798CA5442_DisableCardModeFW=1
//---
FLASH_ECD798CE74C3_ISP=SM3267ACISP-27nm.BIN
FLASH_ECD798CE74C3_PTEST=SM3267ACPTEST.bin
FLASH_ECD798CE74C3_DisableCardModeFW=1
//---
FLASH_2C88044BA900_ISP=SM3267ACISP.BIN
FLASH_2C88044BA900_PTEST=SM3267ACPTEST.bin
FLASH_2C88044BA900_PSCAN=SM3267ACPSCN.bin
FLASH_2C88044BA900_PSCNFlash=3
FLASH_2C88044BA900_DisableCardModeFW=1
//---
//---
FLASH_2C64403CA904_ISP=SM3267ACISP-L84.BIN
FLASH_2C64403CA904_PTEST=SM3267ACPTEST.bin
FLASH_2C64403CA904_DisableCardModeFW=1
//---
FLASH_2C84C13CA904_ISP=SM3267ACISP-L84.BIN
FLASH_2C84C13CA904_PTEST=SM3267ACPTEST.bin
FLASH_2C84C13CA904_DisableCardModeFW=1
//---
FLASH_2C24444BA400_ISP=SM3267ACISP-L84.BIN
FLASH_2C24444BA400_PTEST=SM3267ACPTEST.bin
FLASH_2C24444BA400_PSCAN=SM3267ACPSCN.bin
FLASH_2C24444BA400_PSCNFlash=2
FLASH_2C24444BA400_DisableCardModeFW=1
//---
FLASH_8964444BA900_ISP=SM3267ACISP-L84.BIN
FLASH_8964444BA900_PTEST=SM3267ACPTEST.bin
FLASH_8964444BA900_PSCAN=SM3267ACPSCN.bin
FLASH_8964444BA900_PSCNFlash=2
FLASH_8964444BA900_DisableCardModeFW=1
//---
FLASH_89A825CBA984_ISP=SM3267ACISP-L84.BIN
FLASH_89A825CBA984_PTEST=SM3267ACPTEST.bin
FLASH_89A825CBA984_PSCAN=SM3267ACPSCN.bin
FLASH_89A825CBA984_PSCNFlash=2
FLASH_89A825CBA984_DisableCardModeFW=1
//---
FLASH_8988244BA984_ISP=SM3267ACISP-L84.BIN
FLASH_8988244BA984_PTEST=SM3267ACPTEST.bin
FLASH_8988244BA984_PSCAN=SM3267ACPSCN.bin
FLASH_8988244BA984_PSCNFlash=2
FLASH_8988244BA984_DisableCardModeFW=1
//---
FLASH_2C64444BA900_ISP=SM3267ACISP-L84.BIN
FLASH_2C64444BA900_PTEST=SM3267ACPTEST.bin
FLASH_2C64444BA900_PSCAN=SM3267ACPSCN.bin
FLASH_2C64444BA900_PSCNFlash=2
FLASH_2C64444BA900_DisableCardModeFW=1
//---
FLASH_2C84C54BA900_ISP=SM3267ACISP-L84.BIN
FLASH_2C84C54BA900_PTEST=SM3267ACPTEST.bin
FLASH_2C84C54BA900_PSCAN=SM3267ACPSCN.bin
FLASH_2C84C54BA900_PSCNFlash=2
FLASH_2C84C54BA900_DisableCardModeFW=1
//---
FLASH_2C44444BA900_ISP=SM3267ACISP-L84.BIN
FLASH_2C44444BA900_PTEST=SM3267ACPTEST.bin
FLASH_2C44444BA900_PSCAN=SM3267ACPSCN.bin
FLASH_2C44444BA900_PSCNFlash=2
FLASH_2C44444BA900_DisableCardModeFW=1
//---
FLASH_2C44403CA504_ISP=SM3267ACISP-16K.BIN
FLASH_2C44403CA504_PTEST=SM3267ACPTEST.bin
FLASH_2C44403CA504_DisableCardModeFW=1
//---
FLASH_2C64643CA504_ISP=SM3267ACISP-L85.BIN
FLASH_2C64643CA504_PTEST=SM3267ACPTEST.bin
FLASH_2C64643CA504_PSCAN=SM3267ACPSCN.bin
FLASH_2C64643CA504_PSCNFlash=1
FLASH_2C64643CA504_DisableCardModeFW=1
FLASH_2C64643CA504_AdjustBlock=0
//---
FLASH_2C84E53CA504_ISP=SM3267ACISP-L85.BIN
FLASH_2C84E53CA504_PTEST=SM3267ACPTEST.bin
FLASH_2C84E53CA504_PSCAN=SM3267ACPSCN.bin
FLASH_2C84E53CA504_PSCNFlash=1
FLASH_2C84E53CA504_DisableCardModeFW=1
FLASH_2C84E53CA504_AdjustBlock=0
//---
FLASH_2C64643CA505_ISP=SM3267ACISP-L85.BIN
FLASH_2C64643CA505_PTEST=SM3267ACPTEST.bin
FLASH_2C64643CA505_PSCAN=SM3267ACPSCN.bin
FLASH_2C64643CA505_PSCNFlash=1
FLASH_2C64643CA505_DisableCardModeFW=1
FLASH_2C64643CA505_AdjustBlock=0
//---
FLASH_2C64643CA100_ISP=SM3267ACISP-L85.BIN
FLASH_2C64643CA100_PTEST=SM3267ACPTEST.bin
FLASH_2C64643CA100_PSCAN=SM3267ACPSCN.bin
FLASH_2C64643CA100_PSCNFlash=1
FLASH_2C64643CA100_DisableCardModeFW=1
FLASH_2C64643CA100_AdjustBlock=0
//---
FLASH_2C64643CA508_ISP=SM3267ACISP-L85.BIN
FLASH_2C64643CA508_PTEST=SM3267ACPTEST.bin
FLASH_2C64643CA508_PSCAN=SM3267ACPSCN.bin
FLASH_2C64643CA508_PSCNFlash=1
FLASH_2C64643CA508_DisableCardModeFW=1
FLASH_2C64643CA508_AdjustBlock=0
//---
FLASH_2C846434A500_ISP=SM3267ACISP-L85.BIN
FLASH_2C846434A500_PTEST=SM3267ACPTEST.bin
FLASH_2C846434A500_PSCAN=SM3267ACPSCN.bin
FLASH_2C846434A500_PSCNFlash=0
FLASH_2C846434A500_DisableCardModeFW=1
FLASH_2C846434A500_AdjustBlock=0
//---
FLASH_2C84643CA500_ISP=SM3267ACISP-L85.BIN
FLASH_2C84643CA500_PTEST=SM3267ACPTEST.bin
FLASH_2C84643CA500_PSCAN=SM3267ACPSCN.bin
FLASH_2C84643CA500_PSCNFlash=0
FLASH_2C84643CA500_DisableCardModeFW=1
FLASH_2C84643CA500_AdjustBlock=0
//---
FLASH_2C84643CA904_ISP=SM3267ACISP-L85.BIN
FLASH_2C84643CA904_PTEST=SM3267ACPTEST.bin
FLASH_2C84643CA904_PSCAN=SM3267ACPSCN.bin
FLASH_2C84643CA904_PSCNFlash=0
FLASH_2C84643CA904_DisableCardModeFW=1
FLASH_2C84643CA904_AdjustBlock=0
//---
FLASH_2CA4E53CA904_ISP=SM3267ACISP-L85.BIN
FLASH_2CA4E53CA904_PTEST=SM3267ACPTEST.bin
FLASH_2CA4E53CA904_PSCAN=SM3267ACPSCN.bin
FLASH_2CA4E53CA904_PSCNFlash=0
FLASH_2CA4E53CA904_DisableCardModeFW=1
FLASH_2CA4E53CA904_AdjustBlock=0
//---
FLASH_2C84643CA905_ISP=SM3267ACISP-L85.BIN
FLASH_2C84643CA905_PTEST=SM3267ACPTEST.bin
FLASH_2C84643CA905_PSCAN=SM3267ACPSCN.bin
FLASH_2C84643CA905_PSCNFlash=0
FLASH_2C84643CA905_DisableCardModeFW=1
FLASH_2C84643CA905_AdjustBlock=0
//---
FLASH_2CA4E53CA905_ISP=SM3267ACISP-L85.BIN
FLASH_2CA4E53CA905_PTEST=SM3267ACPTEST.bin
FLASH_2CA4E53CA905_PSCAN=SM3267ACPSCN.bin
FLASH_2CA4E53CA905_PSCNFlash=0
FLASH_2CA4E53CA905_DisableCardModeFW=1
FLASH_2CA4E53CA905_AdjustBlock=0
//---
FLASH_2C846454A900_ISP=SM3267ACISP-L85.BIN
FLASH_2C846454A900_PTEST=SM3267ACPTEST.bin
FLASH_2C846454A900_PSCAN=SM3267ACPSCN.bin
FLASH_2C846454A900_PSCNFlash=0
FLASH_2C846454A900_DisableCardModeFW=1
FLASH_2C846454A900_AdjustBlock=0
//---
FLASH_2C846454A901_ISP=SM3267ACISP-L85.BIN
FLASH_2C846454A901_PTEST=SM3267ACPTEST.bin
FLASH_2C846454A901_PSCAN=SM3267ACPSCN.bin
FLASH_2C846454A901_PSCNFlash=0
FLASH_2C846454A901_DisableCardModeFW=1
FLASH_2C846454A901_AdjustBlock=0
//---
FLASH_2CA4E554A900_ISP=SM3267ACISP-L85.BIN
FLASH_2CA4E554A900_PTEST=SM3267ACPTEST.bin
FLASH_2CA4E554A900_PSCAN=SM3267ACPSCN.bin
FLASH_2CA4E554A900_PSCNFlash=0
FLASH_2CA4E554A900_DisableCardModeFW=1
FLASH_2CA4E554A900_AdjustBlock=0
//---
FLASH_8984643CA500_ISP=SM3267ACISP-L85.BIN
FLASH_8984643CA500_PTEST=SM3267ACPTEST.bin
FLASH_8984643CA500_PSCAN=SM3267ACPSCN.bin
FLASH_8984643CA500_PSCNFlash=0
FLASH_8984643CA500_DisableCardModeFW=1
FLASH_8984643CA500_AdjustBlock=0
//---
FLASH_89A4E53CA500_ISP=SM3267ACISP-L85.BIN
FLASH_89A4E53CA500_PTEST=SM3267ACPTEST.bin
FLASH_89A4E53CA500_PSCAN=SM3267ACPSCN.bin
FLASH_89A4E53CA500_PSCNFlash=0
FLASH_89A4E53CA500_DisableCardModeFW=1
FLASH_89A4E53CA500_AdjustBlock=0
//---
FLASH_8964643CA500_ISP=SM3267ACISP-L85.BIN
FLASH_8964643CA500_PTEST=SM3267ACPTEST.bin
FLASH_8964643CA500_PSCAN=SM3267ACPSCN.bin
FLASH_8964643CA500_PSCNFlash=1
FLASH_8964643CA500_DisableCardModeFW=1
FLASH_8964643CA500_AdjustBlock=0
//---
FLASH_8964643CA100_ISP=SM3267ACISP-L85.BIN
FLASH_8964643CA100_PTEST=SM3267ACPTEST.bin
FLASH_8964643CA100_PSCAN=SM3267ACPSCN.bin
FLASH_8964643CA100_PSCNFlash=1
FLASH_8964643CA100_DisableCardModeFW=1
FLASH_8964643CA100_AdjustBlock=0
//---
FLASH_8964643CA50C_ISP=SM3267ACISP-L85.BIN
FLASH_8964643CA50C_PTEST=SM3267ACPTEST.bin
FLASH_8964643CA50C_PSCAN=SM3267ACPSCN.bin
FLASH_8964643CA50C_PSCNFlash=1
FLASH_8964643CA50C_DisableCardModeFW=1
FLASH_8964643CA50C_AdjustBlock=0
//---
FLASH_8964643CA10C_ISP=SM3267ACISP-L85.BIN
FLASH_8964643CA10C_PTEST=SM3267ACPTEST.bin
FLASH_8964643CA10C_PSCAN=SM3267ACPSCN.bin
FLASH_8964643CA10C_PSCNFlash=1
FLASH_8964643CA10C_DisableCardModeFW=1
FLASH_8964643CA10C_AdjustBlock=0
//---
FLASH_8984643CA50C_ISP=SM3267ACISP-L85.BIN
FLASH_8984643CA50C_PTEST=SM3267ACPTEST.bin
FLASH_8984643CA50C_PSCAN=SM3267ACPSCN.bin
FLASH_8984643CA50C_PSCNFlash=0
FLASH_8984643CA50C_DisableCardModeFW=1
FLASH_8984643CA50C_AdjustBlock=0
//---
FLASH_89C4E63CA50C_ISP=SM3267ACISP-L85.BIN
FLASH_89C4E63CA50C_PTEST=SM3267ACPTEST.bin
FLASH_89C4E63CA50C_PSCAN=SM3267ACPSCN.bin
FLASH_89C4E63CA50C_PSCNFlash=0
FLASH_89C4E63CA50C_DisableCardModeFW=1
FLASH_89C4E63CA50C_AdjustBlock=1
//---
FLASH_8984643CA50C_ISP=SM3267ACISP-L85.BIN
FLASH_8984643CA50C_PTEST=SM3267ACPTEST.bin
FLASH_8984643CA50C_PSCAN=SM3267ACPSCN.bin
FLASH_8984643CA50C_PSCNFlash=0
FLASH_8984643CA50C_DisableCardModeFW=1
FLASH_8984643CA50C_AdjustBlock=0
//---
FLASH_8984643CA90C_ISP=SM3267ACISP-L85.BIN
FLASH_8984643CA90C_PTEST=SM3267ACPTEST.bin
FLASH_8984643CA90C_PSCAN=SM3267ACPSCN.bin
FLASH_8984643CA90C_PSCNFlash=0
FLASH_8984643CA90C_DisableCardModeFW=1
FLASH_8984643CA90C_AdjustBlock=0
//---
FLASH_2C84643CA400_ISP=SM3267ACISP-L85.BIN
FLASH_2C84643CA400_PTEST=SM3267ACPTEST.bin
FLASH_2C84643CA400_PSCAN=SM3267ACPSCN.bin
FLASH_2C84643CA400_PSCNFlash=0
FLASH_2C84643CA400_DisableCardModeFW=1
FLASH_2C84643CA400_AdjustBlock=0
//---
FLASH_2CA4E53CA500_ISP=SM3267ACISP-L85.BIN
FLASH_2CA4E53CA500_PTEST=SM3267ACPTEST.bin
FLASH_2CA4E53CA500_PSCAN=SM3267ACPSCN.bin
FLASH_2CA4E53CA500_PSCNFlash=0
FLASH_2CA4E53CA500_DisableCardModeFW=1
FLASH_2CA4E53CA500_AdjustBlock=0
//---
FLASH_2C846434A400_ISP=SM3267ACISP-L85.BIN
FLASH_2C846434A400_PTEST=SM3267ACPTEST.bin
FLASH_2C846434A400_PSCAN=SM3267ACPSCN.bin
FLASH_2C846434A400_PSCNFlash=0
FLASH_2C846434A400_DisableCardModeFW=1
FLASH_2C846434A400_AdjustBlock=0
//---
FLASH_2CA4E534A500_ISP=SM3267ACISP-L85.BIN
FLASH_2CA4E534A500_PTEST=SM3267ACPTEST.bin
FLASH_2CA4E534A500_PSCAN=SM3267ACPSCN.bin
FLASH_2CA4E534A500_PSCNFlash=0
FLASH_2CA4E534A500_DisableCardModeFW=1
FLASH_2CA4E534A500_AdjustBlock=0
//---
FLASH_2C64643CA400_ISP=SM3267ACISP-L85.BIN
FLASH_2C64643CA400_PTEST=SM3267ACPTEST.bin
FLASH_2C64643CA400_PSCAN=SM3267ACPSCN.bin
FLASH_2C64643CA400_PSCNFlash=1
FLASH_2C64643CA400_DisableCardModeFW=1
FLASH_2C64643CA400_AdjustBlock=0
//---
FLASH_2C84643B8900_ISP=SM3267ACISP-L85.BIN
FLASH_2C84643B8900_PTEST=SM3267ACPTEST.bin
FLASH_2C84643B8900_PSCAN=SM3267ACPSCN.bin
FLASH_2C84643B8900_PSCNFlash=0
FLASH_2C84643B8900_DisableCardModeFW=1
FLASH_2C84643B8900_AdjustBlock=0
//---
FLASH_B584643B8900_ISP=SM3267ACISP-L85.BIN
FLASH_B584643B8900_PTEST=SM3267ACPTEST.bin
FLASH_B584643B8900_PSCAN=SM3267ACPSCN.bin
FLASH_B584643B8900_PSCNFlash=0
FLASH_B584643B8900_DisableCardModeFW=1
FLASH_B584643B8900_AdjustBlock=0
//---
FLASH_B5846454A900_ISP=SM3267ACISP-L85.BIN
FLASH_B5846454A900_PTEST=SM3267ACPTEST.bin
FLASH_B5846454A900_PSCAN=SM3267ACPSCN.bin
FLASH_B5846454A900_PSCNFlash=0
FLASH_B5846454A900_DisableCardModeFW=1
FLASH_B5846454A900_AdjustBlock=0
//---
FLASH_2C646456A500_ISP=SM3267ACISP-L94.BIN
FLASH_2C646456A500_PTEST=SM3267ACPTEST.bin
FLASH_2C646456A500_PSCAN=SM3267ACPSCN.bin
/FLASH_2C646456A500_PSCNFlash=0
FLASH_2C646456A500_DisableCardModeFW=1
FLASH_2C646456A500_AdjustBlock=0
//---
FLASH_2C646456A504_ISP=SM3267ACISP-L94.BIN
FLASH_2C646456A504_PTEST=SM3267ACPTEST.bin
FLASH_2C646456A504_PSCAN=SM3267ACPSCN.bin
/FLASH_2C646456A504_PSCNFlash=0
FLASH_2C646456A504_DisableCardModeFW=1
FLASH_2C646456A504_AdjustBlock=0
//---
FLASH_B584643CA904_ISP=SM3267ACISP-L85.BIN
FLASH_B584643CA904_PTEST=SM3267ACPTEST.bin
FLASH_B584643CA904_DisableCardModeFW=1
//---
FLASH_B5A4E53CA904_ISP=SM3267ACISP-L85.BIN
FLASH_B5A4E53CA904_PTEST=SM3267ACPTEST.bin
FLASH_B5A4E53CA904_DisableCardModeFW=1
//---

//---
FLASH_2C84643B8900_ISP=SM3267ACISP-L85-AL.BIN
FLASH_2C84643B8900_PTEST=SM3267ACPTEST.bin
FLASH_2C84643B8900_PSCAN=SM3267ACPSCN.bin
FLASH_2C84643B8900_DisableCardModeFW=1
//---
FLASH_ECD7943264C5_ISP=SM3267ACISP-SA19nmMLC.BIN
FLASH_ECD7943264C5_PTEST=SM3267ACPTEST.bin
FLASH_ECD7943264C5_DisableCardModeFW=1
//---
FLASH_ECDEA43268C5_ISP=SM3267ACISP-SA19nmMLC.BIN
FLASH_ECDEA43268C5_PTEST=SM3267ACPTEST.bin
FLASH_ECDEA43268C5_DisableCardModeFW=1
//---
FLASH_ECD7947E64C4_ISP=SM3267ACISP-SA21nmMLC.BIN
FLASH_ECD7947E64C4_PTEST=SM3267ACPTEST.bin
FLASH_ECD7947E64C4_DisableCardModeFW=1
//---
FLASH_ECD7947E64C4_ISP=SM3267ACISP-SA21nmMLC.BIN
FLASH_ECD7947E64C4_PTEST=SM3267ACPTEST.bin
FLASH_ECD7947E64C4_DisableCardModeFW=1
//---
FLASH_ECDEA47E78C4_ISP=SM3267ACISP-SA21nmMLC.BIN
FLASH_ECDEA47E78C4_PTEST=SM3267ACPTEST.bin
FLASH_ECDEA47E78C4_DisableCardModeFW=1
//---
FLASH_ECDEA47A68C4_ISP=SM3267ACISP-SA21nmMLC.BIN
FLASH_ECDEA47A68C4_PTEST=SM3267ACPTEST.bin
FLASH_ECDEA47A68C4_DisableCardModeFW=1
//---
FLASH_ECAEA47A68C4_ISP=SM3267ACISP-SA21nmMLC.BIN
FLASH_ECAEA47A68C4_PTEST=SM3267ACPTEST.bin
FLASH_ECAEA47A68C4_DisableCardModeFW=1
//---
FLASH_ECAEA47A68C4_ISP=SM3267ACISP-SA21nmMLC.BIN
FLASH_ECAEA47A68C4_PTEST=SM3267ACPTEST.bin
FLASH_ECAEA47A68C4_DisableCardModeFW=1
//---
FLASH_ECAEA47A68C4_ISP=SM3267ACISP-SA21nmMLC.BIN
FLASH_ECAEA47A68C4_PTEST=SM3267ACPTEST.bin
FLASH_ECAEA47A68C4_DisableCardModeFW=1
//---
FLASH_ECD7947E6444_ISP=SM3267ACISP-SA21nmMLC.BIN
FLASH_ECD7947E6444_PTEST=SM3267ACPTEST.bin
FLASH_ECD7947E6444_DisableCardModeFW=1
//---
FLASH_ECD594765443_ISP=SM3267ACISP-SA27nmMLC.BIN
FLASH_ECD594765443_PTEST=SM3267ACPTEST.bin
FLASH_ECD594765443_DisableCardModeFW=1
//---
FLASH_ECD794766443_ISP=SM3267ACISP-SA27nmMLC.BIN
FLASH_ECD794766443_PTEST=SM3267ACPTEST.bin
FLASH_ECD794766443_DisableCardModeFW=1
//---
FLASH_ECDE95766843_ISP=SM3267ACISP-SA27nmMLC.BIN
FLASH_ECDE95766843_PTEST=SM3267ACPTEST.bin
FLASH_ECDE95766843_DisableCardModeFW=1
//---
FLASH_ECD7947A5443_ISP=SM3267ACISP-SA27nmMLC.BIN
FLASH_ECD7947A5443_PTEST=SM3267ACPTEST.bin
FLASH_ECD7947A5443_DisableCardModeFW=1
//---
FLASH_ECDED57A5843_ISP=SM3267ACISP-SA27nmMLC.BIN
FLASH_ECDED57A5843_PTEST=SM3267ACPTEST.bin
FLASH_ECDED57A5843_DisableCardModeFW=1
//---
FLASH_ECDED5765843_ISP=SM3267ACISP-SA27nmMLC.BIN
FLASH_ECDED5765843_PTEST=SM3267ACPTEST.bin
FLASH_ECDED5765843_DisableCardModeFW=1
//---
FLASH_ECD5947654C3_ISP=SM3267ACISP-SA27nmMLC.BIN
FLASH_ECD5947654C3_PTEST=SM3267ACPTEST.bin
FLASH_ECD5947654C3_DisableCardModeFW=1
//---
FLASH_ECD7947A64C3_ISP=SM3267ACISP-SA27nmMLC.BIN
FLASH_ECD7947A64C3_PTEST=SM3267ACPTEST.bin
FLASH_ECD7947A64C3_DisableCardModeFW=1
//---
FLASH_ECD7947A54C3_ISP=SM3267ACISP-SA27nmMLC.BIN
FLASH_ECD7947A54C3_PTEST=SM3267ACPTEST.bin
FLASH_ECD7947A54C3_DisableCardModeFW=1
//---
FLASH_ECD594765443_ISP=SM3267ACISP-SA27nmMLC.BIN
FLASH_ECD594765443_PTEST=SM3267ACPTEST.bin
FLASH_ECD594765443_DisableCardModeFW=1
//---
FLASH_ECD794765443_ISP=SM3267ACISP-SA27nmMLC.BIN
FLASH_ECD794765443_PTEST=SM3267ACPTEST.bin
FLASH_ECD794765443_DisableCardModeFW=1
//---
FLASH_ECDEA43268C5_ISP=SM3267ACISP-SA19nmMLC.BIN
FLASH_ECDEA43268C5_PTEST=SM3267ACPTEST.bin
FLASH_ECDEA43268C5_DisableCardModeFW=1
//---
FLASH_ECDE94F3A4C6_ISP=SM3267ACISP-SA16nmMLC.BIN
FLASH_ECDE94F3A4C6_PTEST=SM3267ACPTEST.bin
FLASH_ECDE94F3A4C6_DisableCardModeFW=1
//---

//---
FLASH_98D584327256_ISP=SM3267ACISP-24nm.BIN
FLASH_98D584327256_PTEST=SM3267ACPTEST.bin
FLASH_98D584327256_DisableCardModeFW=1
//---
FLASH_98D5843272D6_ISP=SM3267ACISP-24nm.BIN
FLASH_98D5843272D6_PTEST=SM3267ACPTEST.bin
FLASH_98D5843272D6_DisableCardModeFW=1
//---
FLASH_98DE94827656_ISP=SM3267ACISP-24nm.BIN
FLASH_98DE94827656_PTEST=SM3267ACPTEST.bin
FLASH_98DE94827656_DisableCardModeFW=1
//---
FLASH_98D794327656_ISP=SM3267ACISP-24nm.BIN
FLASH_98D794327656_PTEST=SM3267ACPTEST.bin
FLASH_98D794327656_DisableCardModeFW=1
//---
FLASH_98DEA4827656_ISP=SM3267ACISP-24nm.BIN
FLASH_98DEA4827656_PTEST=SM3267ACPTEST.bin
FLASH_98DEA4827656_DisableCardModeFW=1
//---
FLASH_98DE948276D6_ISP=SM3267ACISP-24nm.BIN
FLASH_98DE948276D6_PTEST=SM3267ACPTEST.bin
FLASH_98DE948276D6_DisableCardModeFW=1
//---
FLASH_98D7943276D6_ISP=SM3267ACISP-24nm.BIN
FLASH_98D7943276D6_PTEST=SM3267ACPTEST.bin
FLASH_98D7943276D6_DisableCardModeFW=1
//---
FLASH_98D584327656_ISP=SM3267ACISP-24nm.BIN
FLASH_98D584327656_PTEST=SM3267ACPTEST.bin
FLASH_98D584327656_DisableCardModeFW=1
//---
FLASH_98D5843276D6_ISP=SM3267ACISP-24nm.BIN
FLASH_98D5843276D6_PTEST=SM3267ACPTEST.bin
FLASH_98D5843276D6_DisableCardModeFW=1
//---
FLASH_45D794327656_ISP=SM3267ACISP-24nm.BIN
FLASH_45D794327656_PTEST=SM3267ACPTEST.bin
FLASH_45D794327656_DisableCardModeFW=1
//---
FLASH_45DE94827656_ISP=SM3267ACISP-24nm.BIN
FLASH_45DE94827656_PTEST=SM3267ACPTEST.bin
FLASH_45DE94827656_DisableCardModeFW=1
//---
FLASH_45D584327256_ISP=SM3267ACISP-24nm.BIN
FLASH_45D584327256_PTEST=SM3267ACPTEST.bin
FLASH_45D584327256_DisableCardModeFW=1
//---
FLASH_45D5843272D6_ISP=SM3267ACISP-24nm.BIN
FLASH_45D5843272D6_PTEST=SM3267ACPTEST.bin
FLASH_45D5843272D6_DisableCardModeFW=1
//---
FLASH_45DE948276D6_ISP=SM3267ACISP-24nm.BIN
FLASH_45DE948276D6_PTEST=SM3267ACPTEST.bin
FLASH_45DE948276D6_DisableCardModeFW=1
//---
FLASH_98DEA4827657_ISP=SM3267ACISP-24nm.BIN
FLASH_98DEA4827657_PTEST=SM3267ACPTEST.bin
FLASH_98DEA4827657_DisableCardModeFW=1
//---
FLASH_98DEA48276D7_ISP=SM3267ACISP-24nm.BIN
FLASH_98DEA48276D7_PTEST=SM3267ACPTEST.bin
FLASH_98DEA48276D7_DisableCardModeFW=1
//---
FLASH_983AD6327ED5_ISP=SM3267ACISP-24nm.BIN
FLASH_983AD6327ED5_PTEST=SM3267ACPTEST.bin
FLASH_983AD6327ED5_DisableCardModeFW=1
//---
FLASH_453A97327ED5_ISP=SM3267ACISP-24nm.BIN
FLASH_453A97327ED5_PTEST=SM3267ACPTEST.bin
FLASH_453A97327ED5_DisableCardModeFW=1
//---
FLASH_983AA5827A56_ISP=SM3267ACISP-24nm.BIN
FLASH_983AA5827A56_PTEST=SM3267ACPTEST.bin
FLASH_983AA5827A56_DisableCardModeFW=1
//---
FLASH_452D94827656_ISP=SM3267ACISP-24nm.BIN
FLASH_452D94827656_PTEST=SM3267ACPTEST.bin
FLASH_452D94827656_DisableCardModeFW=1
//---
FLASH_454D94827656_ISP=SM3267ACISP-24nm.BIN
FLASH_454D94827656_PTEST=SM3267ACPTEST.bin
FLASH_454D94827656_DisableCardModeFW=1
//---
FLASH_456D95827A56_ISP=SM3267ACISP-24nm.BIN
FLASH_456D95827A56_PTEST=SM3267ACPTEST.bin
FLASH_456D95827A56_DisableCardModeFW=1
//---
FLASH_45DEA4827656_ISP=SM3267ACISP-24nm.BIN
FLASH_45DEA4827656_PTEST=SM3267ACPTEST.bin
FLASH_45DEA4827656_DisableCardModeFW=1
//---
FLASH_98DEA48276D6_ISP=SM3267ACISP-24nm.BIN
FLASH_98DEA48276D6_PTEST=SM3267ACPTEST.bin
FLASH_98DEA48276D6_DisableCardModeFW=1
//---
FLASH_45DEA4827657_ISP=SM3267ACISP-24nm.BIN
FLASH_45DEA4827657_PTEST=SM3267ACPTEST.bin
FLASH_45DEA4827657_DisableCardModeFW=1
//---
FLASH_45DEA4927657_ISP=SM3267ACISP-24nm.BIN
FLASH_45DEA4927657_PTEST=SM3267ACPTEST.bin
FLASH_45DEA4927657_DisableCardModeFW=1
//---
FLASH_98DE948376D6_ISP=SM3267ACISP-24nm.BIN
FLASH_98DE948376D6_PTEST=SM3267ACPTEST.bin
FLASH_98DE948376D6_DisableCardModeFW=1
//---
FLASH_983A95837AD6_ISP=SM3267ACISP-24nm.BIN
FLASH_983A95837AD6_PTEST=SM3267ACPTEST.bin
FLASH_983A95837AD6_DisableCardModeFW=1
//---
FLASH_453AA5827A56_ISP=SM3267ACISP-24nm.BIN
FLASH_453AA5827A56_PTEST=SM3267ACPTEST.bin
FLASH_453AA5827A56_DisableCardModeFW=1
//---

//---
FLASH_98D7A0327656_ISP=SM3267ACISP.bin
FLASH_98D7A0327656_PTEST=SM3267ACPTEST.bin
FLASH_98D7A0327656_PSCAN=SM3267ACPSCN.bin
FLASH_98D7A0327656_PSCNFlash=11
FLASH_98D7A0327656_DisableCardModeFW=1
//---
FLASH_98DEA1327A56_ISP=SM3267ACISP.bin
FLASH_98DEA1327A56_PTEST=SM3267ACPTEST.bin
FLASH_98DEA1327A56_PSCAN=SM3267ACPSCN.bin
FLASH_98DEA1327A56_PSCNFlash=12
FLASH_98DEA1327A56_DisableCardModeFW=1
//---
FLASH_98D390267615_ISP=SM3267ACISP.bin
FLASH_98D390267615_PTEST=SM3267ACPTEST.bin
FLASH_98D390267615_PSCAN=SM3267ACPSCN.bin
FLASH_98D390267615_PSCNFlash=13
FLASH_98D390267615_DisableCardModeFW=1
//---


//---
FLASH_983AA5827AD7_ISP=SM3267ACISP-T19nmMLC.BIN
FLASH_983AA5827AD7_PTEST=SM3267ACPTEST.bin
FLASH_983AA5827AD7_DisableCardModeFW=1
//---
FLASH_454C86937A57_ISP=SM3267ACISP-ISPSD19nm16K_INTintlv.BIN
FLASH_454C86937A57_PTEST=SM3267ACPTEST.bin
FLASH_454C86937A57_DisableCardModeFW=1
//---
FLASH_453C86937A57_ISP=SM3267ACISP-ISPSD19nm16K_INTintlv.BIN
FLASH_453C86937A57_PTEST=SM3267ACPTEST-iNand.bin
FLASH_453C86937A57_PSCAN=SM3267ACPSCN.bin
FLASH_453C86937A57_PSCNFlash=24
FLASH_453C86937A57_DisableCardModeFW=1
//---
FLASH_45DE84937257_ISP=SM3267ACISP-ISPSD19nm16K.BIN
FLASH_45DE84937257_PTEST=SM3267ACPTEST.bin
FLASH_45DE84937257_DisableCardModeFW=1
//---
FLASH_453A85937657_ISP=SM3267ACISP-ISPSD19nm16K.BIN
FLASH_453A85937657_PTEST=SM3267ACPTEST.bin
FLASH_453A85937657_DisableCardModeFW=1
//---
FLASH_45DE849372D7_ISP=SM3267ACISP-ISPSD19nm16K.BIN
FLASH_45DE849372D7_PTEST=SM3267ACPTEST.bin
FLASH_45DE849372D7_DisableCardModeFW=1
//---
FLASH_98DE84937257_ISP=SM3267ACISP-ISPT19nm16K.BIN
FLASH_98DE84937257_PTEST=SM3267ACPTEST.bin
FLASH_98DE84937257_DisableCardModeFW=1
//---
FLASH_98DE849372D7_ISP=SM3267ACISP-ISPT19nm16K.BIN
FLASH_98DE849372D7_PTEST=SM3267ACPTEST.bin
FLASH_98DE849372D7_DisableCardModeFW=1
//---
FLASH_983A85937657_ISP=SM3267ACISP-ISPT19nm16K.BIN
FLASH_983A85937657_PTEST=SM3267ACPTEST.bin
FLASH_983A85937657_DisableCardModeFW=1
//---
FLASH_983A859376D7_ISP=SM3267ACISP-ISPT19nm16K.BIN
FLASH_983A859376D7_PTEST=SM3267ACPTEST.bin
FLASH_983A859376D7_DisableCardModeFW=1

//---
FLASH_98DE94937657_ISP=SM3267ACISP-ISPT19nm16K.BIN
FLASH_98DE94937657_PTEST=SM3267ACPTEST.bin
FLASH_98DE94937657_DisableCardModeFW=1
//---
FLASH_98DE949376D7_ISP=SM3267ACISP-ISPT19nm16K.BIN
FLASH_98DE949376D7_PTEST=SM3267ACPTEST.bin
FLASH_98DE949376D7_DisableCardModeFW=1
//---
FLASH_983A95937AD7_ISP=SM3267ACISP-ISPT19nm16K.BIN
FLASH_983A95937AD7_PTEST=SM3267ACPTEST.bin
FLASH_983A95937AD7_DisableCardModeFW=1
//---
FLASH_983A95937A57_ISP=SM3267ACISP-ISPT19nm16K.BIN
FLASH_983A95937A57_PTEST=SM3267ACPTEST.bin
FLASH_983A95937A57_DisableCardModeFW=1
//---
FLASH_983A95937A57_ISP=SM3267ACISP-ISPT19nm16K.BIN
FLASH_983A95937A57_PTEST=SM3267ACPTEST.bin
FLASH_983A95937A57_DisableCardModeFW=1
//---
FLASH_98D7849372D7_ISP=SM3267ACISP-ISPT19nm16K.BIN
FLASH_98D7849372D7_PTEST=SM3267ACPTEST.bin
FLASH_98D7849372D7_DisableCardModeFW=1
//---
FLASH_98D784937257_ISP=SM3267ACISP-ISPT19nm16K.BIN
FLASH_98D784937257_PTEST=SM3267ACPTEST.bin
FLASH_98D784937257_DisableCardModeFW=1
//---
FLASH_45DE94937657_ISP=SM3267ACISP-ISPSD19nm16K.BIN
FLASH_45DE94937657_PTEST=SM3267ACPTEST.bin
FLASH_45DE94937657_DisableCardModeFW=1
//---
FLASH_45DE949376D7_ISP=SM3267ACISP-ISPSD19nm16K.BIN
FLASH_45DE949376D7_PTEST=SM3267ACPTEST.bin
FLASH_45DE949376D7_DisableCardModeFW=1
//---
FLASH_453AA4937A50_ISP=SM3267ACISP-ISPSD1ynm16K.BIN
FLASH_453AA4937A50_PTEST=SM3267ACPTEST.bin
FLASH_453AA4937A50_DisableCardModeFW=1
//---
FLASH_453AA4937AD0_ISP=SM3267ACISP-ISPSD1ynm16K.BIN
FLASH_453AA4937AD0_PTEST=SM3267ACPTEST.bin
FLASH_453AA4937AD0_DisableCardModeFW=1
//---
FLASH_45DE94937650_ISP=SM3267ACISP-ISPSD1ynm16K.BIN
FLASH_45DE94937650_PTEST=SM3267ACPTEST.bin
FLASH_45DE94937650_DisableCardModeFW=1
//---
FLASH_45DE949376D0_ISP=SM3267ACISP-ISPSD1ynm16K.BIN
FLASH_45DE949376D0_PTEST=SM3267ACPTEST.bin
FLASH_45DE949376D0_DisableCardModeFW=1
//---
FLASH_983A95937A50_ISP=SM3267ACISP-ISPT1ynm16K.BIN
FLASH_983A95937A50_PTEST=SM3267ACPTEST.bin
FLASH_983A95937A50_DisableCardModeFW=1
//---
FLASH_983A95937AD0_ISP=SM3267ACISP-ISPT1ynm16K.BIN
FLASH_983A95937AD0_PTEST=SM3267ACPTEST.bin
FLASH_983A95937AD0_DisableCardModeFW=1
//---
FLASH_98D784937250_ISP=SM3267ACISP-ISPT1ynm16K.BIN
FLASH_98D784937250_PTEST=SM3267ACPTEST.bin
FLASH_98D784937250_DisableCardModeFW=1
//---
FLASH_98DE94937650_ISP=SM3267ACISP-ISPT1ynm16K.BIN
FLASH_98DE94937650_PTEST=SM3267ACPTEST.bin
FLASH_98DE94937650_DisableCardModeFW=1
//---
FLASH_98DE949376D0_ISP=SM3267ACISP-ISPT1ynm16K.BIN
FLASH_98DE949376D0_PTEST=SM3267ACPTEST.bin
FLASH_98DE949376D0_DisableCardModeFW=1
//---
FLASH_983AA4937A50_ISP=SM3267ACISP-ISPT1ynm16K.BIN
FLASH_983AA4937A50_PTEST=SM3267ACPTEST.bin
FLASH_983AA4937A50_DisableCardModeFW=1
//---
FLASH_983AA4937AD0_ISP=SM3267ACISP-ISPT1ynm16K.BIN
FLASH_983AA4937AD0_PTEST=SM3267ACPTEST.bin
FLASH_983AA4937AD0_DisableCardModeFW=1
//---
FLASH_983CA5937E50_ISP=SM3267ACISP-ISPT1ynm16K.BIN
FLASH_983CA5937E50_PTEST=SM3267ACPTEST.bin
FLASH_983CA5937E50_DisableCardModeFW=1
//---
FLASH_983CA5937ED0_ISP=SM3267ACISP-ISPT1ynm16K.BIN
FLASH_983CA5937ED0_PTEST=SM3267ACPTEST.bin
FLASH_983CA5937ED0_DisableCardModeFW=1
//---
FLASH_98DE94937651_ISP=SM3267ACISP-ISPT15nm16K.BIN
FLASH_98DE94937651_PTEST=SM3267ACPTEST.bin
FLASH_98DE94937651_DisableCardModeFW=1
//---
FLASH_98DE949376D1_ISP=SM3267ACISP-ISPT15nm16K.BIN
FLASH_98DE949376D1_PTEST=SM3267ACPTEST.bin
FLASH_98DE949376D1_DisableCardModeFW=1
//---
FLASH_983A94937651_ISP=SM3267ACISP-ISPT15nm16K.BIN
FLASH_983A94937651_PTEST=SM3267ACPTEST.bin
FLASH_983A94937651_DisableCardModeFW=1
//---
FLASH_983A949376D1_ISP=SM3267ACISP-ISPT15nm16K.BIN
FLASH_983A949376D1_PTEST=SM3267ACPTEST.bin
FLASH_983A949376D1_DisableCardModeFW=1
//---
FLASH_983C95937A51_ISP=SM3267ACISP-ISPT15nm16K.BIN
FLASH_983C95937A51_PTEST=SM3267ACPTEST.bin
FLASH_983C95937A51_DisableCardModeFW=1
//---
FLASH_983C95937AD1_ISP=SM3267ACISP-ISPT15nm16K.BIN
FLASH_983C95937AD1_PTEST=SM3267ACPTEST.bin
FLASH_983C95937AD1_DisableCardModeFW=1
//---
FLASH_453A94937651_ISP=SM3267ACISP-ISPSD15nm16K.BIN
FLASH_453A94937651_PTEST=SM3267ACPTEST.bin
FLASH_453A94937651_DisableCardModeFW=1
//---
FLASH_453A949376D1_ISP=SM3267ACISP-ISPSD15nm16K.BIN
FLASH_453A949376D1_PTEST=SM3267ACPTEST.bin
FLASH_453A949376D1_DisableCardModeFW=1
//---
FLASH_ADDE18030040_ISP=SM3267ACISP-ISPHYTLC.BIN
FLASH_ADDE18030040_PTEST=SM3267ACPTEST.bin
FLASH_ADDE18030040_DisableCardModeFW=1
//---
FLASH_AD3A18A36125_ISP=SM3267ACISP-ISPHYTLC.BIN
FLASH_AD3A18A36125_PTEST=SM3267ACPTEST.bin
FLASH_AD3A18A36125_DisableCardModeFW=1
//---
FLASH_AD3A18A361E5_ISP=SM3267ACISP-ISPHYTLC.BIN
FLASH_AD3A18A361E5_PTEST=SM3267ACPTEST.bin
FLASH_AD3A18A361E5_DisableCardModeFW=1
//---
FLASH_ADD594DA74C4_ISP=SM3267ACISP-HY.BIN
FLASH_ADD594DA74C4_PTEST=M3267ACPTEST.bin
FLASH_ADD594DA74C4_PSCAN=SM3267ACPSCN.bin
FLASH_ADD594DA74C4_HYEN=IESLCEN.BIN
FLASH_ADD594DA74C4_HYDS=IESLCDS.BIN
FLASH_ADD594DA74C4_DisableCardModeFW=1
//---
FLASH_ADD794DA74C3_ISP=\HY-8K\SM3267ACISP-HY.BIN
FLASH_ADD794DA74C3_PTEST=SM3267ACPTEST.bin
FLASH_ADD794DA74C3_PSCAN=SM3267ACPSCN.bin
FLASH_ADD794DA74C3_HYEN=\HY-8K\IESLCEN.BIN
FLASH_ADD794DA74C3_HYDS=\HY-8K\IESLCDS.BIN
FLASH_ADD794DA74C3_DisableCardModeFW=1
//---
FLASH_ADDE94D20443_ISP=SM3267ACISP-HY.BIN
FLASH_ADDE94D20443_PTEST=SM3267ACPTEST.bin
FLASH_ADDE94D20443_PSCAN=SM3267ACPSCN.bin
FLASH_ADDE94D20443_HYEN=IESLCEN.BIN
FLASH_ADDE94D20443_HYDS=IESLCDS.BIN
FLASH_ADDE94D20443_DisableCardModeFW=1
//---
FLASH_ADDE94DA74C4_ISP=SM3267ACISP-HY.BIN
FLASH_ADDE94DA74C4_PTEST=SM3267ACPTEST.bin
FLASH_ADDE94DA74C4_PSCAN=SM3267ACPSCN.bin
FLASH_ADDE94DA74C4_HYEN=IESLCEN.BIN
FLASH_ADDE94DA74C4_HYDS=IESLCDS.BIN
FLASH_ADDE94DA74C4_DisableCardModeFW=1
//---
FLASH_ADD794916044_ISP=SM3267ACISP-HY.BIN
FLASH_ADD794916044_PTEST=SM3267ACPTEST.bin
FLASH_ADD794916044_PSCAN=SM3267ACPSCN.bin
FLASH_ADD794916044_HYEN=IESLCEN.BIN
FLASH_ADD794916044_HYDS=IESLCDS.BIN
FLASH_ADD794916044_DisableCardModeFW=1
//---
FLASH_ADD7149E344A_ISP=SM3267ACISP-HY.BIN
FLASH_ADD7149E344A_PTEST=SM3267ACPTEST.bin
FLASH_ADD7149E344A_HYEN=IESLCEN.BIN
FLASH_ADD7149E344A_HYDS=IESLCDS.BIN
FLASH_ADD7149E344A_DisableCardModeFW=1
//--- 8T2BYR
FLASH_ADDE94EB7444_ISP=SM3267ACISP-ISPHY20nm.BIN
FLASH_ADDE94EB7444_PTEST=SM3267ACPTEST.bin
FLASH_ADDE94EB7444_PSCAN=SM3267ACPSCN.bin
FLASH_ADDE94EB7444_PSCNFlash=16
FLASH_ADDE94EB7444_HYEN=iESLCEN.BIN
FLASH_ADDE94EB7444_HYDS=iESLCDS.BIN
FLASH_ADDE94EB7444_DisableCardModeFW=1
//---
FLASH_AD3A95EB7844_ISP=SM3267ACISP-ISPHY20nm.BIN
FLASH_AD3A95EB7844_PTEST=SM3267ACPTEST.bin
FLASH_AD3A95EB7844_PSCAN=SM3267ACPSCN.bin
FLASH_AD3A95EB7844_PSCNFlash=16
FLASH_AD3A95EB7844_HYEN=iESLCEN.BIN
FLASH_AD3A95EB7844_HYDS=iESLCDS.BIN
FLASH_AD3A95EB7844_DisableCardModeFW=1
//---
FLASH_ADDE94974445_ISP=SM3267ACISP-ISPHY20nm.BIN
FLASH_ADDE94974445_PTEST=SM3267ACPTEST.bin
FLASH_ADDE94974445_PSCAN=SM3267ACPSCN.bin
FLASH_ADDE94974445_PSCNFlash=17
FLASH_ADDE94974445_HYEN=iESLCEN.BIN
FLASH_ADDE94974445_HYDS=iESLCDS.BIN
FLASH_ADDE94974445_DisableCardModeFW=1
//---
FLASH_ADDE14A7424A_ISP=SM3267ACISP-ISPHY20nm.BIN
FLASH_ADDE14A7424A_PTEST=SM3267ACPTEST.bin
FLASH_ADDE14A7424A_PSCAN=SM3267ACPSCN.bin
FLASH_ADDE14A7424A_PSCNFlash=17
FLASH_ADDE14A7424A_HYEN=iESLCEN.BIN
FLASH_ADDE14A7424A_HYDS=iESLCDS.BIN
FLASH_ADDE14A7424A_DisableCardModeFW=1
//---
FLASH_AD3A15A7444A_ISP=SM3267ACISP-ISPHY20nm.BIN
FLASH_AD3A15A7444A_PTEST=SM3267ACPTEST.bin
FLASH_AD3A15A7444A_PSCAN=SM3267ACPSCN.bin
FLASH_AD3A15A7444A_PSCNFlash=17
FLASH_AD3A15A7444A_HYEN=iESLCEN.BIN
FLASH_AD3A15A7444A_HYDS=iESLCDS.BIN
FLASH_AD3A15A7444A_DisableCardModeFW=1
//---
FLASH_AD3A14AB424A_ISP=SM3267ACISP-ISPHY20nm.BIN
FLASH_AD3A14AB424A_PTEST=SM3267ACPTEST.bin
FLASH_AD3A14AB424A_PSCAN=SM3267ACPSCN.bin
FLASH_AD3A14AB424A_PSCNFlash=17
FLASH_AD3A14AB424A_HYEN=iESLCEN.BIN
FLASH_AD3A14AB424A_HYDS=iESLCDS.BIN
FLASH_AD3A14AB424A_DisableCardModeFW=1
//---
FLASH_AD3C15AB444A_ISP=SM3267ACISP-ISPHY20nm.BIN
FLASH_AD3C15AB444A_PTEST=SM3267ACPTEST.bin
FLASH_AD3C15AB444A_PSCAN=SM3267ACPSCN.bin
FLASH_AD3C15AB444A_PSCNFlash=17
FLASH_AD3C15AB444A_HYEN=iESLCEN.BIN
FLASH_AD3C15AB444A_HYDS=iESLCDS.BIN
FLASH_AD3C15AB444A_DisableCardModeFW=1
//---
FLASH_ADDE14AB424A_ISP=SM3267ACISP-ISPHY20nm.BIN
FLASH_ADDE14AB424A_PTEST=SM3267ACPTEST.bin
FLASH_ADDE14AB424A_DisableCardModeFW=1
//---
FLASH_ADDE17AA424A_ISP=SM3267ACISP-ISPHY20nm.BIN
FLASH_ADDE17AA424A_PTEST=SM3267ACPTEST.bin
FLASH_ADDE17AA424A_PSCAN=SM3267ACPSCN.bin
FLASH_ADDE17AA424A_PSCNFlash=17
FLASH_ADDE17AA424A_HYEN=iESLCEN.BIN
FLASH_ADDE17AA424A_HYDS=iESLCDS.BIN
FLASH_ADDE17AA424A_DisableCardModeFW=1
//---
FLASH_AD3A15A7444A_ISP=SM3267ACISP-ISPHY20nm.BIN
FLASH_AD3A15A7444A_PTEST=SM3267ACPTEST.bin
FLASH_AD3A15A7444A_PSCAN=SM3267ACPSCN.bin
FLASH_AD3A15A7444A_PSCNFlash=17
FLASH_AD3A15A7444A_HYEN=iESLCEN.BIN
FLASH_AD3A15A7444A_HYDS=iESLCDS.BIN
FLASH_AD3A15A7444A_DisableCardModeFW=1
//---
FLASH_50504E010006_ISP=SM3267ACE2NISP.BIN
FLASH_50504E010006_PTEST=SM3267ACPTEST.bin
FLASH_50504E010006_DisableCardModeFW=1
//---
FLASH_50504E010003_ISP=SM3267ACE2NISP.BIN
FLASH_50504E010003_PTEST=SM3267ACPTEST.bin
FLASH_50504E010003_DisableCardModeFW=1
//---
FLASH_50504E010505_ISP=SM3267ACE2NISP.BIN
FLASH_50504E010505_PTEST=SM3267ACPTEST.bin
FLASH_50504E010505_DisableCardModeFW=1
//---
//---
FLASH_AD8201220141_ISP=SM3267ACE2NISP.BIN
FLASH_AD8201220141_PTEST=SM3267ACPTEST.bin
FLASH_AD8201220141_DisableCardModeFW=1
//---
FLASH_AD8201220142_ISP=SM3267ACE2NISP.BIN
FLASH_AD8201220142_PTEST=SM3267ACPTEST.bin
FLASH_AD8201220142_DisableCardModeFW=1
//---
FLASH_AD8252232101_ISP=SM3267ACE2NISP.BIN
FLASH_AD8252232101_PTEST=SM3267ACPTEST.bin
FLASH_AD8252232101_DisableCardModeFW=1
//---
FLASH_AD8252232102_ISP=SM3267ACE2NISP.BIN
FLASH_D8252232102_PTEST=SM3267ACPTEST.bin
FLASH_D8252232102_DisableCardModeFW=1
//---
FLASH_AD8252232104_ISP=SM3267ACE2NISP.BIN
FLASH_AD8252232104_PTEST=SM3267ACPTEST.bin
FLASH_AD8252232104_DisableCardModeFW=1
//---
FLASH_AD8251232144_ISP=SM3267ACE2NISP.BIN
FLASH_AD8251232144_PTEST=SM3267ACPTEST.bin
FLASH_AD8251232144_DisableCardModeFW=1
//---
FLASH_AD8252232108_ISP=SM3267ACE2NISP.BIN
FLASH_AD8252232108_PTEST=SM3267ACPTEST.bin
FLASH_AD8252232108_DisableCardModeFW=1
//---
FLASH_980004161401_ISP=SM3267ACE2NISP.BIN
FLASH_980004161401_PTEST=SM3267ACPTEST.bin
FLASH_980004161401_DisableCardModeFW=1
//---
FLASH_980004181402_ISP=SM3267ACE2NISP.BIN
FLASH_980004181402_PTEST=SM3267ACPTEST.bin
FLASH_980004181402_DisableCardModeFW=1
//---
FLASH_9800041A1404_ISP=SM3267ACE2NISP.BIN
FLASH_9800041A1404_PTEST=SM3267ACPTEST.bin
FLASH_9800041A1404_DisableCardModeFW=1
FLASH_9800041A1404_AdjustBlock=1
//---
FLASH_980001281502_ISP=SM3267ACE2NISP.BIN
FLASH_980001281502_PTEST=SM3267ACPTEST.bin
FLASH_980001281502_DisableCardModeFW=1
//---
FLASH_980001261502_ISP=SM3267ACE2NISP.BIN
FLASH_980001261502_PTEST=SM3267ACPTEST.bin
FLASH_980001261502_DisableCardModeFW=1
//---
FLASH_980001281504_ISP=SM3267ACE2NISP.BIN
FLASH_980001281504_PTEST=SM3267ACPTEST.bin
FLASH_980001281504_DisableCardModeFW=1
//---
FLASH_9800012A1508_ISP=SM3267ACE2NISP.BIN
FLASH_9800012A1508_PTEST=SM3267ACPTEST.bin
FLASH_9800012A1508_DisableCardModeFW=1
FLASH_9800012A1508_AdjustBlock=1
//---
FLASH_458260DE5702_ISP=SM3267ACE2NISP.BIN
FLASH_458260DE5702_PTEST=SM3267ACPTEST.bin
FLASH_458260DE5702_DisableCardModeFW=1
//---
FLASH_458260DE5704_ISP=SM3267ACE2NISP.BIN
FLASH_458260DE5704_PTEST=SM3267ACPTEST.bin
FLASH_458260DE5704_DisableCardModeFW=1
//---
FLASH_458260DE5708_ISP=SM3267ACE2NISP.BIN
FLASH_458260DE5708_PTEST=SM3267ACPTEST.bin
FLASH_458260DE5708_DisableCardModeFW=1
//---
FLASH_AD8260242101_ISP=SM3267ACE2NISP.BIN
FLASH_AD8260242101_PTEST=SM3267ACPTEST.bin
FLASH_AD8260242101_DisableCardModeFW=1
//---
FLASH_AD8260242102_ISP=SM3267ACE2NISP.BIN
FLASH_AD8260242102_PTEST=SM3267ACPTEST.bin
FLASH_AD8260242102_DisableCardModeFW=1
//---
FLASH_AD8260242104_ISP=SM3267ACE2NISP.BIN
FLASH_AD8260242104_PTEST=SM3267ACPTEST.bin
FLASH_AD8260242104_DisableCardModeFW=1
//---
FLASH_AD8260242108_ISP=SM3267ACE2NISP.BIN
FLASH_AD8260242108_PTEST=SM3267ACPTEST.bin
FLASH_AD8260242108_DisableCardModeFW=1
//---

//---
FLASH_453CA6827E56_ISP=SM3267ACISPINTintlv.BIN
FLASH_453CA6827E56_PTEST=SM3267ACPTEST.bin
FLASH_453CA6827E56_DisableCardModeFW=1
//---
FLASH_453EA7827E56_ISP=SM3267ACISPINTintlv.BIN
FLASH_453EA7827E56_PTEST=SM3267ACPTEST.bin
FLASH_453EA7827E56_DisableCardModeFW=1
//---
FLASH_453E87937E57_ISP=SM3267ACISP-ISPSD19nm16K.BIN
FLASH_453E87937E57_PTEST=SM3267ACPTEST.bin
FLASH_453E87937E57_DisableCardModeFW=1
FLASH_453E87937E57_AdjustBlock=1
//---

//---------------------------------------------------------------------//
FLASH_98DE94937657_RETRY=Sorting_T_SRTY19nmMLC.bin
FLASH_98DE84937257_RETRY=Sorting_T_SRTY19nmMLC.bin
FLASH_983A94937651_RETRY=Sorting_T_SRTY15nmMLC.bin
FLASH_98DE94937651_RETRY=Sorting_T_SRTY15nmMLC.bin
FLASH_983AA4937A50_RETRY=Sorting_T_SRTY1ynmMLC.bin
FLASH_98de94937650_RETRY=Sorting_T_SRTY1ynmMLC.bin
FLASH_98DE98927250_RETRY=Sorting_T_SRTY1ynmTLC.bin
FLASH_983AA8927650_RETRY=Sorting_T_SRTY1ynmTLC.bin
FLASH_ADD744DA74C3_RETRY=Sorting_SRTYHY.bin
FLASH_ADDE14A7424A_RETRY=Sorting_SRTYHY.bin
FLASH_ADDE94EB7444_RETRY=Sorting_SRTYHY.bin
FLASH_ADD794DA74C3_RETRY=Sorting_SRTYHY.bin
FLASH_AD3A14AB424A_RETRY=Sorting_SRTYHY.bin
FLASH_ADDE14AB424A_RETRY=Sorting_SRTYHY.bin

FLASH_AD3A18A36125_RETRY=Sorting_SRTYHYTLC.bin
FLASH_ECDE98DE94C5_RETRY=Sorting_Samsung_SRTY19NM.bin
FLASH_2C64444BA900_RETRY=Sorting_SRTYL84.bin
FLASH_2C84C54BA900_RETRY=Sorting_SRTYL84.bin
FLASH_453A94937651_RETRY=Sorting_SD_SRTY15nmMLC.bin
FLASH_45DE84937257_RETRY=Sorting_SD_SRTY19nmMLC.bin
FLASH_45DEA4927657_RETRY=Sorting_SD_SRTY19nmMLC.bin
FLASH_45DE94937657_RETRY=Sorting_SD_SRTY19nmMLC.bin
FLASH_453AA4937A50_RETRY=Sorting_SD_SRTY1ynmMLC.bin
FLASH_45de94937650_RETRY=Sorting_SD_SRTY1ynmMLC.bin
FLASH_454C98A37651_RETRY=Sorting_SD_SRTY15nmTLC.bin
FLASH_2C64643CA100_RETRY=Sorting_SRTYL85.bin
FLASH_2C64643CA400_RETRY=Sorting_SRTYL85.bin
FLASH_2C64643CA504_RETRY=Sorting_SRTYL85.bin
FLASH_2C64643CA505_RETRY=Sorting_SRTYL85.bin
FLASH_2C84E53CA504_RETRY=Sorting_SRTYL85.bin
FLASH_8964643CA100_RETRY=Sorting_SRTYL85.bin
FLASH_8964643CA10C_RETRY=Sorting_SRTYL85.bin
FLASH_8964643CA500_RETRY=Sorting_SRTYL85.bin
FLASH_8964643CA50C_RETRY=Sorting_SRTYL85.bin
FLASH_B544643CA004_RETRY=Sorting_SRTYL85.bin
FLASH_B564643CA504_RETRY=Sorting_SRTYL85.bin
FLASH_2C64643CA508_RETRY=Sorting_SRTYL85.bin
FLASH_2C846434A500_RETRY=Sorting_SRTYL85.bin
FLASH_2C84643B8900_RETRY=Sorting_SRTYL85.bin
FLASH_2C84643CA400_RETRY=Sorting_SRTYL85.bin
FLASH_2C84643CA500_RETRY=Sorting_SRTYL85.bin
FLASH_2CA4E534A500_RETRY=Sorting_SRTYL85.bin
FLASH_2CA4E53CA500_RETRY=Sorting_SRTYL85.bin
FLASH_8984643CA500_RETRY=Sorting_SRTYL85.bin
FLASH_89A4E53CA500_RETRY=Sorting_SRTYL85.bin
FLASH_B584643B8900_RETRY=Sorting_SRTYL85.bin
FLASH_B584643CA500_RETRY=Sorting_SRTYL85.bin
FLASH_2C84643CA904_RETRY=Sorting_SRTYL85.bin
FLASH_2C84643CA905_RETRY=Sorting_SRTYL85.bin
FLASH_2CA4E53CA904_RETRY=Sorting_SRTYL85.bin
FLASH_2CA4E53CA905_RETRY=Sorting_SRTYL85.bin
FLASH_8984643CA50C_RETRY=Sorting_SRTYL85.bin
FLASH_8984643CA90C_RETRY=Sorting_SRTYL85.bin
FLASH_89A4E53CA50C_RETRY=Sorting_SRTYL85.bin
FLASH_89C4E63CA50C_RETRY=Sorting_SRTYL85.bin
FLASH_B564643CA004_RETRY=Sorting_SRTYL85.bin
FLASH_B584643CA904_RETRY=Sorting_SRTYL85.bin
FLASH_B5A4E53CA904_RETRY=Sorting_SRTYL85.bin
FLASH_2C846454A900_RETRY=Sorting_SRTYL85.bin
FLASH_2C846454A901_RETRY=Sorting_SRTYL85.bin
FLASH_2CA4E554A900_RETRY=Sorting_SRTYL85.bin
FLASH_2CA4E554A901_RETRY=Sorting_SRTYL85.bin
FLASH_B5646454A400_RETRY=Sorting_SRTYL85.bin
FLASH_B5846454A900_RETRY=Sorting_SRTYL85.bin